**LIMITED TENDER ENQUIRY**

**BIT/PUR/LTE/EEE/20-21//IC00423/2020 DATE: 28/12/2020**

To,

**M/s. ..............................................**

Dear Sir,

Subject: Request for Quotation for Procurement of AC VOLTMETER 0-500V etc.

You are requested to submit most competitive rates(s) for the following item(s) as per details given below (Sealed Quotations may be sent by hand or by post):

|  |  |
| --- | --- |
| Last date and time for submissions of complete Quotations by  Email to [dr.purchase@bitmesra.ac.in](mailto:dr.purchase@bitmesra.ac.in),  [purchase.suman@bitmesra.ac.in](mailto:purchase.suman@bitmesra.ac.in) sealed quotations can be submitted to the under mentioned address. | **06.01.2021 15:00 Hrs.**  ( If all LTE Vendors submit the quotation prior to the submission date, the quotations will be opened prior to last date of submission.) |
| Date /time and place for opening of quotation | **06.01.2021**  **16:00 Hrs Purchase Section.** |

|  |  |  |
| --- | --- | --- |
| Sr.No. | Item Description | **Quantity** |
| 1 | AC VOLTMETER 0-500V :  Portable Analog ,BenchtypeVoltmeter - 0 - 500 v  Usage = Laboratory, Portable in ABS body & Wooden Box, | **02 Nos.** |
| 2 | AC VOLTMETER 0-25 V :  Portable Analog ,BenchtypeVoltmeter - 0-25 V  Usage = Laboratory, Portable in ABS body & Wooden Box, | **02 Nos.** |
| 3 | AC/DC VOLTMETER 0-300 V : AC/DC VOLTMETER =Portable Analog ,Bench type  AC/DC VOLTMETER= Range 0-300 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **02 Nos.** |
| 4 | DC VOLTMETER 0-250 V : DC VOLTMETER =Portable Analog ,Bench type Voltmeter = 0-250 V  Usage = Laboratory, Portable in ABS body & Wooden Box, | **02 Nos.** |
| 5 | DC VOLTMETER 0-15 V : DC VOLTMETER =Portable Analog ,Bench Type Voltmeter = 0-15V  Usage = Laboratory, Portable in ABS body & Wooden Box, | **02 Nos.** |
| 6 | DC AMMETER RANGE 0-1 A : DC AMMETER =Portable Analog ,Bench type DC  Ammeter Range 0-1 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **05 Nos.** |
| 7 | DC AMMETER RANGE 0-20 A : DC AMMETER =Portable Analog ,Bench type DC  Ammeter Range 0-20 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **02 Nos** |
| 8 | AC/DC AMMETER 0-30A : AC/DC AMMETER =Portable Analog ,Bench type  AC/DC Ammeter Range 0-30 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **02 Nos** |
| 9 | AC AMMETER RANGE 0-5A : AC AMMETER =Portable Analog ,Bench type Ac  Ammeter Range 0-5 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **02 Nos** |
| 10 | AC AMMETER RANGE 0-10A : AC AMMETER =Portable Analog ,Bench type  Ac Ammeter Range 0-10 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **02 Nos** |
| 11 | AC AMMETER RANGE 0-20 A : AC AMMETER =Portable Analog ,Bench type Ac  Ammeter Range 0-20 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **02 Nos** |
| 12 | AC AMMETER 0-30A : AC AMMETER =Portable Analog ,Bench type Ac  Ammeter Range 0-30 A  Usage = Laboratory, Portable in ABS body & Wooden Box | **02 Nos** |
| 13 | DOUBLE BARREL RHEOSTATE 480 OHM 2A :  RHEOSTATE = DOUBLE BARREL RHEOSTATE 480  OHM 2A, Usage = Laboratory,Q- Saw, Brass Make. | **05 Nos** |
| 14 | DOUBLE BARREL RHEOSTATE 200 OHM 2.8A :  RHEOSTATE = DOUBLE BARREL RHEOSTATE 200  OHM 2.8A, Usage = Laboratory,Q- Saw, Brass Make. | **05 Nos** |
| 15 | SINGLE BARREL RHEOSTATE 300 OHM 1.5A :  RHEOSTATE= SINGLE BARREL RHEOSTATE 300  OHM 1.5A, Usage = Laboratory,Q- Saw, Brass Make. | **05 Nos** |
| 16 | PHASE SEQUENCE METER 3 PHASE 440V, 50HZ : | **01 Nos** |
| 17 | 1-PHASE WATTMETER 150/300/600V, 5/10A : | **02 Nos** |
| 18 | 1-PHASE WATTMETER,150/300/600V,10/20A : | **02 Nos** |
| 19 | 3-PHASE AUTOTRANSFORMER0-,400V/0-480V10 KVA: 3-PHASE AUTOTRANSFORMER0-,400V/0-480V10 KVA  INPUT -415V AC,OUTPUT - 0-470V, 3PH AC ,  # - Phase, 50Hz, Capacity: 10 KVA (output - input Port Upper side) | **02 Nos** |
| 20 | LAMP LOAD, 1-PHASE 250V 2KW : LAMP LOAD, 1-PHASE 250V 2KW  Usage = Laboratory, Portable in ABS body & Wooden box, | **03 Nos** |
| 21 | LAMP LOAD 3-PHASE 440V 2.4KW : Usage = Laboratory, Portable in ABS body & Wooden Box, | **03 Nos** |

Sealed Quotation may be submitted superscribed with reference number as appended hereunder:-

|  |
| --- |
| Quotation for Supply of ----  Ref.No. -------- **BIT/PUR/LTE/EEE/20-21//IC00423/2020**-------------------------------------------------  To,  Additional Registrar (Finance)  Birla Institute of Technology From : M/s----------------------------------------  Mesra , Ranchi , Jharkhand Address : ----------------------------------------  835215 Contact No. -------------------------------------  Email ID--------------------------------------- |

GST Exemption: The Institute is partially exempted from the payment  
of GST vide GOI Notification No.45/2017-Central Tax (Rate), dated  
14.11.2017 and 47/2017-Integrated Tax (Rate), dated: 14.11.2017 the applicable IGST will be at the rate of 5%. Necessary documents (DSIR) and related certification will be provided.

1. All entries in the quotation should be typed or computer printed without any ambiguity and should be free from correction etc. Hand written offers will be rejected.
2. Late and delayed tenders will not be considered. In case any unscheduled holiday occurs on prescribed closing date the next working day shall be the prescribed date of closing.
3. The quotation should be submitted with descriptive literature & drawing. The make of the items offered should be clearly specified.
4. Material should be confirming to our specification. The deviations if any should be clearly indicated in the quotations.
5. Successful bidder has to furnish the OEM test certificates along with the materials (if applicable).
6. Rate /Price: The offered price shall be on **FOR BIT Mesra on Door Delivery basis**.
7. If offered Price Term is other than the FOR-Destination term, approximate Freight & forwarding charges along with the applicable Insurance charges may be mentioned.
8. Details of GST registration, PAN No. should be furnished along with quotations.
9. Purchaser will not pay separately for transit insurance/taxes (if any) and the supplier will be responsible until the stores arrive in good condition at the destination.
10. Warranty: Period of warranty should be clearly mentioned and also the parts covered under it. Warranty will be applicable from the date of successful installation.
11. Service Facility: Supplier must mention about the service set up in India & confirm effective after sales service.
12. BIT Mesra is not bound to accept the lowest or any quotation for whatsoever reason and reserve its right to accept or reject in whole or in part any or all the quotations received without assigning any reason.
13. Applicable taxes shall be quoted separately for all items and levies payable by the supplier under the contract shall be included in the unit price.

Each bidder shall submit only one quotation and sealed quotation to be submitted / delivered at the address. (Alternatively it can be email at [dr.purchase@bitmesra.ac.in](mailto:dr.purchase@bitmesra.ac.in), ar.[purchase1@bitmesra.ac.in](mailto:purchase1@bitmesra.ac.in) / [purchase.suman@bitmesra.ac.in](mailto:purchase.suman@bitmesra.ac.in), or deliver by hand.

1. Training clause ( if any )to be mentioned.
2. Delivery period should be mentioned clearly in the quotation.
3. Conditional tenders will not be considered.
4. Authorized dealership certificate should be submitted in case principal manufacturing company is not quoting directly.

Sd/-

Deputy Registrar Purchase

BIT Mesra Ranchi-835215